**Annex No. 1 to Request for Proposal 3/ZR/IDŚ**

**Bid Form**

|  |
| --- |
| **THE BID****TASTA Armatura Sp. z o.o.** **ul. Grabskiego 38****37-450 Stalowa Wola***Stamp of the Contractor*In the proceedings for the award of a public contract conducted under the Competitive Procedure No. 3/ZR/IDŚ**entitled** **"Supply of specialized hydraulic press for the process of hydroforming of elements for collectors in the range of DN250 to DN600 mm along with instrumentation".** |
| 1. **CONTRACTOR'S DATA:**

Person authorized to represent the Contractor(s) and signing the bid:Contractor(s): Address:**NIP (Tax Identification Number):** **REGON (National Business Registry Number):** **CONTRACTOR is a small / medium entrepreneur - yes □ no □.****CONTRACTOR comes from a European Union member state other than Poland - yes □ no □.****CONTRACTOR comes from another Member State which is not a member of the European Union - yes □ no □****● Delete as appropriate, mark yes or no with X**Person responsible for contact with the Ordering Party: Contact details to which correspondence related to this procedure should be forwarded: **E- MAIL:** Correspondence address (if different from the registered office address):  |
| 1. **TOTAL BID PRICE:**

*I hereby offer to perform the subject matter of the order for the TOTAL BID PRICE\*\*\*nia za ŁĄCZNĄ CENĘ OFERTOWĄ\*\*riumma w rozdziale III SIWZmacją o podstawie do dysponowania tymi osobami, konania zamówienia, a:*Net: ……………………………………………………. [ ] PLN [ ] EURO [ ] USD [[1]](#footnote-1)VAT: …………………………………………………….Gross: …………………………………………………… |
| 1. **We offer a device that meets the following parameters:**

|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Description of the subject matter of the order** | **Required value** | **Offered value** |
| 1. | Processing size range | 10''-24'' inches |  |
| 2. | Total cylinder force | 90,000 kN |  |
| 3. | Max. forming force (max. reinforcement force) | 2350 bar |  |
| 4. | Main cylinder pressure | 30,000 kN |  |
| 5. | Return stroke force of the main cylinder  | 1850 kN |  |
| 6. | Max light (max distance between moving beam and work table) | 2400 mm |  |
| 7. | Stroke of the main cylinder | 1100 mm |  |
| 8. | Rapid lowering speed of the clamping cylinder | ~80 m/s |  |
| 9. | Feeding speed of the clamping cylinder | 5-10 m/s |  |
| 10. | Return speed of the clamping cylinder | ~80 m/s |  |
| 11. | Actual upward sliding block size | 2500x400 mm |  |
| 12. | Actual working table size | 2000x2000 mm |  |
| 13. | Maximum pressure of the hydraulic system | ~25 MPa |  |
| 14. | Side cylinder pressure | 2x28500 kN |  |
| 15. | Stroke of the side cylinder  | 500 mm |  |
| 16. | Ejection force | 3000 kN |  |
| 17. | Ejection stroke | 600 mm |  |
| 18. | Pushing speed of the side cylinder | 5 mm/s |  |
| 19. | Return speed of the side cylinder | ~50 m/s |  |
| 20. | Left and right cylinder synchronization error | ±0.3 mm |  |
| 21. | Size of side sliding blocks | 1000x900 mm |  |
| 22. | Max distance between two side sliding blocks | 2700 mm |  |
| 23. | Center height of molds | 700 mm |  |
| 24. | PLC power supply | SCHNEIDER |  |
| 25. | Electrical components | SCHNEIDER |  |
| 26. | Operation mode | Manual and automatic |  |
| 27. | Total dimension | ~9500x4950x10410 mm |  |
| 28. | System | Full servo system |  |
| 29. | Quick mold change device | YES |  |
| 30. | Remote monitoring and maintenance of the system | YES |  |
| 31. | Total power | ~330 kW |  |
| 32. | Gross weight | ~400 tons |  |

 |
| 1. **We undertake to provide a warranty for the supplied device of the length:**

D.1 Warranty for hydraulic press for hydroforming process................... months |
| **DECLARATIONS:****I declare that**1. the order will be completed within the deadlines specified in the Request for Proposal and in the model contract;
2. the price of our bid includes all costs of order execution;
3. we are acquainted with the Request for Proposal and the model contract and we do not raise any objections to them and we accept the conditions contained therein;
4. we consider ourselves bound by this bid for a period of **30 days** counting from the date of opening of tenders (including this day);
5. we accept the presented model contract without reservation

I have fulfilled the information obligations provided for in Article 13 or Article 14 of the GDPR1) to natural persons from whom I have directly or indirectly obtained personal data in order to apply for the order in question[[2]](#footnote-2).1. I/we have the authorizations, knowledge and experience to perform the subject order,
2. I/we have at our disposal technical potential and persons capable of performing the order,
3. I/we are in an economic and financial situation ensuring the execution of the order,
4. all information included in the bid is up-to-date and true,
 |
| 1. **OBLIGATIONS IN CASE OF AWARDING THE CONTRACT:**
2. we undertake to conclude a contract at a place and date designated by the Ordering Party;
3. the person authorized to contact the Ordering Party in matters relating to the execution of the contract is:

First and last name:e-mail:tel.: |
| 1. **Declaration of No Conflict of Interest**

**I declare that** * 1. **I am/I am not**[[3]](#footnote-3) an entity related personally or by capital to the Ordering Party.

*A capital or personal relationship means a mutual relationship between the Ordering Party or persons authorized to incur liabilities on behalf of the Ordering Party, or persons performing activities on behalf of the Ordering Party related to the contractor selection procedure, and the contractor, consisting in particular of:* 1. *participating in a company as a partner in a civil partnership or a partnership, holding at least 10% of shares (unless a lower threshold is required by law), serving as a member of a supervisory or management body, proxy, attorney;*
2. *being married, in a relationship of kinship or affinity in a direct line, kinship or affinity in a collateral line to the second degree, or a relationship of adoption, custody or guardianship, or having a common life with the contractor, his legal deputy or members of the management or supervisory bodies of the contractors applying for the contract;*
3. *remaining with the contractor in such a legal or factual relationship that there is a reasonable doubt as to their impartiality or independence in connection with the procurement procedure.*
	1. **I am/I am not**[[4]](#footnote-4) an entity with respect to which any of the circumstances indicated in Article 7 of the Law of 13 April 2022 on special solutions to prevent support for aggression against Ukraine and to protect national security apply.
 |
| 1. **TABLE OF CONTENTS:**

The following documents are an integral part of the bid:1. .........................................................................................................................................................
2. .........................................................................................................................................................
3. .........................................................................................................................................................
4. .........................................................................................................................................................

The bid has been submitted on.............. sequentially numbered pages. |
| ……………………………………………………….stamp of the Contractor | ......................................................................................Date and signature of an authorized representative of the Contractor |

1. Mark the appropriate currency [↑](#footnote-ref-1)
2. If the contractor does not provide personal data other than those directly concerning him, or there is an exclusion of the application of the information obligation pursuant to Article 13(4) or Article 14(5) of the GDPR, the content of the statement is not submitted by the contractor (delete the content of the statement, e.g., by crossing it out). [↑](#footnote-ref-2)
3. Delete as needed [↑](#footnote-ref-3)
4. Delete as needed [↑](#footnote-ref-4)